This firmware update should be installed using the Universal Program
Loader software. AG02 firmware can only be installed in the ADU5.  
The Universal Program Loader is available on the Thales Navigation FTP site 
(ftp://ftp.magellangps.com/OEM, Sensor & ADU/utility software).

Magellan programs are designed to operate with industry standard
personal computers.  Use of computers which are not 100% compatible 
with these standards may cause abnormal program operation.

To load firmware with Universal Program Loader:

1.  Place firmware file, fld_fw.bin, in a directory on hard drive.
2.  Connect the receiver to the PC and power on.
3.  Start UPL.  Select to load 'Firmware of the receiver'.
4.  Using browse window select fld_fw.bin.
5.  Select COM port and click on LOAD.
NOTE:  Do not power down the receiver or disconnect from the serial port until 
the program notifies the user that Loading is Complete.  The process will take up 
to five minutes, and the bar showing loading progess will appear to stop for 
various periods of time.  
 

DIRECT ANY QUESTIONS OR PROBLEMS TO TECHNICAL SUPPORT:
Magellan GPS VOICE: 800-229-2400 OPT 2 in North America 
or  408-615-3970 OPT 2 worldwide.  FAX: 408-615-5200   
E-MAIL: oemsupport@magellangps.com
Europe, Middle East and Africa Voice: 33 2 2809 39 24, 
E-Mail: oemsupportemea@magellangps.com
Pacific Rim E-Mail: oemsupportapac@magellangps.com




  
