This HIGH flash memory version of ZG05 can only be loaded into the ZX or ZXW 
Eurorcard or the ZXW or ZX Sensor with boot code 1A01.  The boot code is the 
last field prior to the check sum in the response to query $PASHQ,RID. 
ZG05 firmware update should be installed using the Universal Program Loader 
version 2.30 or higher.  The Universal Program Loading Software is available 
in the OEM, Sensor & ADU/Utility Software folder on the Magellan FTP site at 
ftp://ftp.magellangps.com. 


Magellan s/w programs are designed to operate with industry standard 
personal computers.  Use of computers which are not 100% compatible 
with these standards may cause abnormal program operation.

To load firmware with Universal Program Loader: 

1. Place firmware in directory on hard drive.
2. Connect and power the receiver to the PC.
3. Start program, using browse window select hmzcode.bin
4. Click on OPEN.
5. Select COM port and click on LOAD.
6. Issue command $PASHS,INI,5,5,5,5,1,0 for ZXW Eurocard or ZXW Sensor
without external memory or $PASHS,INI,5,5,5,5,3,0 FOR ZXW Sensor with 
external memory.

DIRECT ANY QUESTIONS OR PROBLEMS TO TECHNICAL SUPPORT:
Americas and worldwide:  (408)615-3980 or (North America Only) 
1-800-229-2400, option 2,
EMAIL: oemsupport@magellangps.com
Europe, Middle East and Africa and worldwide: 33 2 2809 39 24 
EMAIL:  oemsupportemea@magellangps.com
Pacific Rim EMAIL:  oemsupportapac@magellangps.com.  

