Field notes from February 15, 2004

ZMax serial number PROTO1003 used as Stop&Go base

SiteID:  BASE	Recording interval 5 seconds	ZMax with GPS antenna on top (no vortex)

Vertical height to ARP:  5.584 US Feet

ZMax serial number 200335018 used as Stop&Go rover

SiteID:  (file name)  PS03

The first occupation of LOC1 has a bad antenna height with bad PDOP.  SV21 was blocked by the office bldg.  Stayed on LOC1 for 25 minutes to try to overcome the PDOP.

Correct antenna height on LOC1 = 5.584 US Feet

See OPUS report on BASE.

