

# FORWARD/BACKWARD

< Backward Processing >	:	N


# AUTO RESET

< Auto reset mode >	:	0
#	0 means no auto resets
#	1 means whole RTK reset including KF reset, base coordinates, baseline coordinates, hardware biases calibration.
#	2 means whole KF reset
#	3 means position&ambiguity reset only
#	4 means Soft Kalman Filter reset
< Time out interval, seconds >	:	300


# FIXING AMBIGUITY

< Never fix ambiguity before, seconds >	:	0
< Always fix ambiguity after, seconds >	:	2147483647


# BLOCKS DECIMATION

< Decimation of L2 data epochs >	:	1
< Decimation of code data epochs  >	:	1


# DATA CONTAMINATION

< Simulate Code Outliers >	:	N
< Simulate Carrier Cycle Slips >	:	N
