
  

 Data Sheet Retrieval 

The NGS Data SheetSee file  dsdata.txt for more information about the datasheet.
DATABASE =  ,PROGRAM = datasheet, VERSION = 7.85
1        National Geodetic Survey,   Retrieval Date = JULY 24, 2010
 DF4639 ***********************************************************************
 DF4639  DESIGNATION -  OLYMPIC
 DF4639  PID         -  DF4639
 DF4639  STATE/COUNTY-  UT/SALT LAKE
 DF4639  USGS QUAD   -  FORT DOUGLAS (1975)
 DF4639
 DF4639                         *CURRENT SURVEY CONTROL
 DF4639  ___________________________________________________________________
 DF4639* NAD 83(2007)-  40 45 32.75708(N)    111 50 41.20721(W)     ADJUSTED  
 DF4639* NAVD 88     -      1435.8    (meters)    4711.     (feet)  GPS OBS   
 DF4639  ___________________________________________________________________
 DF4639  EPOCH DATE  -        2002.00
 DF4639  X           -  -1,800,624.891 (meters)                     COMP
 DF4639  Y           -  -4,491,699.205 (meters)                     COMP
 DF4639  Z           -   4,143,122.647 (meters)                     COMP
 DF4639  LAPLACE CORR-          13.98  (seconds)                    DEFLEC09
 DF4639  ELLIP HEIGHT-        1419.232 (meters)          (02/10/07) ADJUSTED
 DF4639  GEOID HEIGHT-         -16.52  (meters)                     GEOID09
 DF4639
 DF4639  ------- Accuracy Estimates (at 95% Confidence Level in cm) --------
 DF4639  Type    PID    Designation                      North   East  Ellip
 DF4639  -------------------------------------------------------------------
 DF4639  NETWORK DF4639 OLYMPIC                           0.78   0.51   1.35
 DF4639  -------------------------------------------------------------------
 DF4639
 DF4639.The horizontal coordinates were established by GPS observations
 DF4639.and adjusted by the National Geodetic Survey in February 2007.
 DF4639
 DF4639.The datum tag of NAD 83(2007) is equivalent to NAD 83(NSRS2007).
 DF4639.See National Readjustment for more information.
 DF4639.The horizontal coordinates are valid at the epoch date displayed above.
 DF4639.The epoch date for horizontal control is a decimal equivalence
 DF4639.of Year/Month/Day.
 DF4639
 DF4639.The orthometric height was determined by GPS observations and a
 DF4639.high-resolution geoid model.
 DF4639
 DF4639.Photographs are available for this station.
 DF4639
 DF4639.The X, Y, and Z were computed from the position and the ellipsoidal ht.
 DF4639
 DF4639.The Laplace correction was computed from DEFLEC09 derived deflections.
 DF4639
 DF4639.The ellipsoidal height was determined by GPS observations
 DF4639.and is referenced to NAD 83.
 DF4639
 DF4639.The geoid height was determined by GEOID09.
 DF4639
 DF4639;                    North         East     Units Scale Factor Converg.
 DF4639;SPC UT C     - 2,269,375.194   470,885.759   MT  1.00002897   -0 13 15.1
 DF4639;SPC UT C     - 7,445,441.78  1,544,897.69   sFT  1.00002897   -0 13 15.1
 DF4639;UTM  12      - 4,512,358.561   428,694.293   MT  0.99966258   -0 33 05.6
 DF4639
 DF4639!             -  Elev Factor  x  Scale Factor =   Combined Factor
 DF4639!SPC UT C     -   0.99977742  x   1.00002897  =   0.99980639
 DF4639!UTM  12      -   0.99977742  x   0.99966258  =   0.99944008
 DF4639
 DF4639                          SUPERSEDED SURVEY CONTROL
 DF4639
 DF4639  NAD 83(1994)-  40 45 32.75679(N)    111 50 41.20679(W) AD(       ) 1
 DF4639  ELLIP H (03/31/03) 1419.243  (m)                       GP(       ) 4 2
 DF4639
 DF4639.Superseded values are not recommended for survey control.
 DF4639.NGS no longer adjusts projects to the NAD 27 or NGVD 29 datums.
 DF4639.See file dsdata.txt to determine how the superseded data were derived.
 DF4639
 DF4639_U.S. NATIONAL GRID SPATIAL ADDRESS: 12TVL2869412358(NAD 83)
 DF4639_MARKER: DD = SURVEY DISK
 DF4639_SETTING: 7 = SET IN TOP OF CONCRETE MONUMENT
 DF4639_STAMPING: SALT LAKE 2002
 DF4639_MARK LOGO: NOAA  
 DF4639_PROJECTION: FLUSH
 DF4639_MAGNETIC: O = OTHER; SEE DESCRIPTION
 DF4639_STABILITY: B = PROBABLY HOLD POSITION/ELEVATION WELL
 DF4639_SATELLITE: THE SITE LOCATION WAS REPORTED AS SUITABLE FOR
 DF4639+SATELLITE: SATELLITE OBSERVATIONS - October 07, 2002
 DF4639
 DF4639  HISTORY     - Date     Condition        Report By
 DF4639  HISTORY     - 20021007 MONUMENTED       SLCS
 DF4639
 DF4639                          STATION DESCRIPTION
 DF4639
 DF4639'DESCRIBED BY SALT LAKE COUNTY SURVEYOR 2002 (VEB)
 DF4639'THE STATION IS LOCATED ON THE UNIVERSITY OF UTAH CAMPUS, SALT LAKE
 DF4639'CITY UTAH. MARK IS A 10 IN DIAMETER COMMEMORATIVE OLYMPIC BRASS SET IN
 DF4639'A 2FT DIAMETER CONCRETE CYLINDIRCAL MONUMENT, 5FT DEEP IN THE GROUND.
 DF4639' 
 DF4639'TO REACH THE STATION FROM THE JUNCTION OF INTERSTATE 80 AND INTERSTATE
 DF4639'15, GO EAST 5.5 MILES ON INTERSTATE 80, TO THE FOOTHILL BLVD EXIT,
 DF4639'THEN GO NORTH ON FOOTHILL BLVD (HWY 186 WEST) 4.2 MILES TO 1580 EAST
 DF4639'CAMPUS CENTER ROAD, TURN RIGHT AND GO 150 FT. MONUMENT IS 75 FT EAST
 DF4639'OF THE EAST CURB ON TOP OF A GRASS KNOLL, AT GROUND LEVEL.
 DF4639' 
 DF4639'

 *** retrieval complete.
 Elapsed Time = 00:00:00

